**S K ENTERPRISES**

Specialist in: all interior and exterior work etc.

**Office: Noble house shop no 7 mumbra Devi road mumbra opposite to mumbra railway station mumbra Thane 400613 contact number : 8828653451**

**Date:-04/09/2024**

**Quotation**

**To,**

**Copper chimney viman nagar pune**

**SUB: Quotation for techno commercial offer for MNGL gas pipeline system.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr.No** | **Description** | **Qty** | **Rates** | **Amount** |
|  1 | 40 mm x SCH40 Seamless Pipe SA106 GR "B" ISMT as Inclusive of Pressure Testing And Supports, One Coat of Anticorrosive Primer And two Coats of Yellow Color oil paint and Elbow, tee, clamp etc. Working:- PNG Gas is moved through pipeline as a result of a series of compressors craetinjg pressure differentials\_ Gas Flow from high pressure to relatively low pressure | 12mtrs | 1150 | 13800 |
|  2 | Ball Valve WCB Socket welded Size 40 mm BSPF Working:- A ball valve is a flow control device which uses a hollow, perforated and pivoting ball to control fluid flowing through it. | 1nos | 4320 | 4320 |
| 3 | Ball Valve WCB Brass Body Size 15 mm BSPF Working:- A ball valve is a flow control device which uses a hollow, perforated and pivoting ball to control fluid flowing through it. | 4nos | 650 | 2600 |
| 4 | Burner Pigtail ⅜" Brass Fittings X 4 Ft Long BPT x BPT Working:- Burner pigtails are used to connect cylinder adapters to manifold | 4nos | 520 | 2080 |
| 5 | Pressure Guage 4" Dia 0 - 5000 mmwc with Isolation Valve. Working:- Pressure Guage is used to measure the pressure of gas. | 2nos | 3340 | 6680 |
| 6 | Burner Conversion Charges | 5nos | 370 | 1850 |
| 7 | Third Party Inspection Certificate Charges | 1nos | 14340 | 14340 |
| 8 | Installation, Transportation, Testing & Comissioning Charges | 1 | 10200 | 10200 |
|  |  |
| **Total Amount** | **55870.00** |